arXiv:1302.6044v1 [physics.data-an] 25 Feb 2013

Digital Cavities and Their Potential Applications

Khadga Karki^a, Magne Torbjörsson^a, Julia R. Widom^b, Andrew H. Marcus^b, and Tönu Pullerits^a a Chemical Physics, Lund University, Getingevägen 60, 22241, Lund, Sweden b University of Oregon, Eugene, OR 97403-1253, USA E-mail: Khadga.Karki@chemphys.lu.se

February 26, 2013

Abstract

The concept of a digital cavity is presented. The functionality of a tunable radio-frequency/microwave cavity with unrestricted Q-factor is implemented. The theoretical aspects of the cavity and its potential applications in high resolution spectroscopy and synchronization of clocks together with examples in signal processing and data acquisition are discussed.

1 Introduction

The development of analog to digital converters (ADC) is advancing rapidly. The cutting-edge ADCs available commercially have a bandwidth of 20 GHz and can digitize signals at astonishing speed of about 65 GS/s (giga samples per second). This rapid development in ADCs have enabled analysis of the signals from DC to microwave frequencies digitally.

Traditionally resonator circuits (LC circuits) and cavity resonators have been used to analyze high frequency signals. The resonance frequency of an

LC circuit can be tuned, which makes them useful in applications where the receiver needs the flexibility to analyze signals coming at different frequencies. However, due to the inherent power losses in the circuit the quality factor (Q-factor) that can be achieved in an LC circuit is only about 10^2. Radio frequency cavities or microwave cavities, made up of a closed metal structure that confine electromagnetic field can have extremely high Q-factor (upto 10^6). Each cavity has a set of resonant modes (normal modes) that are determined by the physical parameters of the cavity. These are not easy to tune without compromising the performance of the cavity. Digital cavities overcome the limitation of these resonators, i.e. they are tunable, and at the same time, can have extremely high Q-factor.

In the simple case of a linear cavity formed by two reflecting surfaces, the mode spacing or the free spectral range fsr is given by fsr = c 2L , (1)

where c is the speed of light and L is the distance between the surfaces. The frequencies of the normal modes are given by N · fsr with N ∈ {1, 2, 3, ..}. A sinusoidal signal at the resonance frequency is amplified by the cavity due to constructive interference in the successive round trips in the cavity while the other signals are suppressed due to destructive interference. A timeperiodic boundary condition applied to a sinusoidal signal leads to similar interference effects mimicking the functionality of a cavity. Here, we use the term time-periodic boundary condition to emphasize that the condition applied is similar to the periodic boundary condition (in spatial dimensions) used for example in molecular dynamics simulations [1, 2, 3] to simulate properties of a large system by tessellation of a smaller simulation box. The periodic-boundary condition in time is implemented by translating the signal x(t) at time t to x(t + k · T ), where T is the period and k ∈ {0, 1, 2, ...}. Implementation of such a boundary condition during the digitization of a signal by an ADC leads to the formation of a digital cavity.

Fig.1 shows a pictorial representation of a digital cavity implemented using discrete values of digitized signals. In the figure the signal is discretized at a fixed interval of Δt. A period of the digital cavity contains n = 10 data points with period T = n · Δt. Sinusoidal signals that are in resonance and off-resonance with the cavity are shown in panel (a) and (b), respectively.

Figure 1: Digital cavity with n = 10 and cavity length T = 10Δt. In (a) the signal is resonant with the cavity while it is non-resonant in (b).

2 Theory

A digital cavity of length n is defined as y(j · Δt; n) := N_c∑

k=0 x(j · Δt + k · T ); j = 1, 2, ...n, (2) where the waveform y is the response of the cavity to the signal x and N_c + 1 is the number of times the cavity function is applied to the signal. The cavity defined by Equ.(2) amplifies the resonant frequencies while suppressing (or filtering out) the non-resonant frequencies.

The fundamental mode of the cavity is given by f_0 = 1/(n · Δt), which can be tuned either by changing n or Δt. In an analogous way a physical cavity can be tuned either by changing the cavity length or the dielectric constant of the medium in the cavity. The free spectral range of a digital cavity is the same as the fundamental mode (fsr = f_0), hence the cavity amplifies a frequency comb [4] with frequencies that are integer multiple of the fundamental mode, i.e. f_0, 2f_0, 3f_0, ... including the DC signal as shown in Fig.2. We denote the resonant frequencies by f_{res}. Note that a DC signal is also amplified by an analog cavity. The DC offset of a signal in a digital cavity can be filtered out using a high band pass filter or an AC coupling prior to digitization. Another simple approach to filter out the DC offset is to use a generalized digital cavity as defined later.

The upper limit of the response of the cavity to a non-resonant frequency

Figure 2: A frequency comb that is amplified by a digital cavity. The x-axis is presented as frequency coordinate relative to the fundamental mode. The amplification as well as the line width of the resonant modes depend on N_c.

f is given by ||y(j · Δt)|| ≤ √ 5 2π f_{res} f − f_{res} , (3)

where f_{res} is the resonant frequency closest to f (see Appendix for the derivation), and the norm in the left side of the equation is taken to be the absolute value of the waveform. As shown by Equ.(3) there is no upper bound for resonant frequencies. In this case the waveform gets amplified linearly with N_c, i.e. ||y(j · Δt)|| = (N_c + 1)||x(j · Δt)||, and the cavity response can be made arbitrarily large by choosing N_c appropriately. If we define the amplitude of the response of the cavity to a signal as A(f) = max(||y(j · Δt)||) then the ratio of the amplitude for a resonant frequency to a non-resonant frequency, A(f_{res})/A(f), can be arbitrarily large. This, in other words, means that the line-width of the cavity can be arbitrarily small. We take full-width at half the maximum (FWHM) as the measure of the line-width. Let ξ_{f0} denote the half-width at half the maximum. Then for f = f_0 + ξ_{f0} we have A(f) = (N_c + 1)/2, and using Equ.(3) we get

2ξ_{f0} = 2 √ 5 π(N_c + 1)

. (4)

As the waveform generated after the cavity, y(j · Δt), is a set of numbers, the definition of the amplitude can be generalized. If the amplitude is defined

Figure 3: Line-width of a digital cavity using r = 2 and different values of N_c. The line-width narrows progressively with increasing N_c. The figure also shows that at certain non-resonant frequencies, indicated as nodes, the cavity completely suppresses the signal.

as A(f) = max(||(y(j · Δ))^r||), where r ≥ 1, then the generalized FWHM is given by

2ξ_{f0} = 2^{1/r} √ 5 π(N_c + 1)

. (5)

As shown by Equ.(5) the line-width of a digital cavity can be made arbitrarily narrow by choosing large N_c, and in addition it can also be digitally narrowed by simply choosing larger r. Fig.3 shows line-widths for a digital cavity with different values of N_c and r = 2.

Fig.3 also shows nodes at certain frequencies at which a digital cavity completely suppresses the signal even for low values of N_c. The frequencies at which these nodes occur depend on N_c, and they occur at f = f_{res} + pf_0/(N_c + 1) for p ∈ {1, 2, ..., N_c}. As pointed out later these nodes can be useful in demultiplexing a signal that is multiplexed over different frequencies.

3 Discussion on the Applications and Scope

One of the scientific applications of a digital cavity is in phase-sensitive signal detection. We developed the concept for real time analysis of phase and amplitude of different frequencies present in the fluorescence signal from a sample that is excited with phase modulated laser pulses as in the fluorescence detected wave-packet interferometry [5, 6] and the two-dimensional electronic coherence spectroscopy. [7] In these experiments, the fluorescence from the sample is multiplexed over many frequencies due to the contribution of the linear and the non-linear response of the sample. The signals at different frequencies provide a plethora of information about the system being investigated. A data-acquisition system that is capable of de-multiplexing the different contributions simultaneously would make this technique promising for chemical imaging. This in conjunction with near-field scanning techniques, can provide detailed information of chemical composition of a system with sub-wavelength resolution. [8] A digital cavity can be used to de-multiplex the signal and analyze the different contributions simultaneously. Thus, it could enable multiplexed chemical imaging using the fluorescence detected interferometric techniques. Fig.4 shows two signals at 4 and 6 kHz (panels (b) and (c), respectively) recovered from a signal that is synthesized by digitally mixing four frequencies at 4, 5, 6 and 7 kHz. The signal is digitized at the rate of 96 kS/s (kilo samples per second). Two digital cavities with n = 24 and 16 are implemented in real time to recover the two different contributions to the signal. Other contributions can also be recovered at the same time simply by implementing other cavities with different cavity lengths.

De-multiplexing technique as shown in Fig.4 can also be used in data transmission employing multiple frequencies. When the frequencies are well defined, even small values of N_c can select the signal contribution from the desired frequency. The 4 kHz signal in Fig.4 is selected by using N_c = 3 and the 6 kHz signal is selected by using N_c = 5. Note that for the 4 kHz signal all the other frequencies, 5,6 7 kHz, lie on the nodes of the cavity response when N_c = 3, i.e. they are completely suppressed, and the same is true for the 6 kHz contribution when N_c = 5. Multiplexed data transmission can dramatically improve the data transfer rate compared to the transmission using single frequency as is commonly done in wireless communication. Clever implementation of digital cavities can have significant impact in this field.

A digital cavity described by Equ.(2) is generalization of coherent sampling technique [9, 10] in which a common reference clock is used for signal generation as well as for digitization. Coherent sampling has been used for phase-sensitive detection, similar to that shown in Fig.4, of signals mainly at f_0 and 2f_0 to investigate rare gases using high-resolution tunable diode laser spectroscopy. [10] A digital cavity is generalization of the previously

Figure 4: Signal de-multiplexing using a digital cavity. Panel (a) shows the signal that is generated using direct digital synthesis by summing signals at frequencies 4, 5, 6 and 7 kHz. All the frequencies have same amplitude and zero phase offset. The signal in (a) is digitized using an ADC at a rate of 96 kS/s. A digital cavity with n = 24 selects the signal at 4 kHz (panel (b)) and another cavity with n = 16 selects the signal at 6 kHz (panel(c)). N_c is set to 3 and 5 in (b) and (c), respectively. All the waveforms have been normalized by the maximum value.

implemented techniques in that it does not need the same reference clock for signal generation and digitization. Furthermore the definition of the digital cavity can be generalized as y(j · Δt) := N_c∑

k=0 x(j · Δt + n · Δt · k) cos(k · θ)+ N_c∑

k=0 x((j + l) · Δt + n · Δt · k) sin(k · θ), (6)

where l ∈ {n/4, n/2, 1, 2, 3, ..} is used to offset the fundamental frequency f_0 to f_g = nf_0/(4l), and θ = 2πk(4l −n)/(4l) (see Appendix for the derivation). Equ.(2) is a special case of the generalized cavity in which 4l = n . For 4l = 2n the generalized cavity functions as a comb-pass filter amplifying signals at f_0/2, 3f_0/2, 5f_0/2, ..., and for other l it acts as a comb-pass filter amplifying signals at f_g, f_g + f_0, f_g + 2f_0, .... Note that a DC offset of a signal in the generalized cavity, except for the case when 4l = n, becomes non-resonant with the cavity. The generalized digital cavity can be tuned by changing either of Δt, n or l. Such tunability significantly increases the scope of a digital cavity compared to previously known techniques like the coherent sampling.

As a digital cavity is freely tunable to signal source(s) at a particular frequency it can be used in applications like software defined radio in which the tuning of the radio to a certain frequency is done by the software. When a signal needs to be transmitted over a noisy channel then the cavity can be used to suppress the random (white) noise. Note that the cavity averages a cycle of the resonant signal N_c times, which improves the signal to noise ratio by a factor of √ N_c for the random noise. Fig.5 shows two sinusoidal signals retrieved from their corresponding noisy parent signals. Some examples where suppression of white noise becomes important is in signal transmission over long distance (satellite communication, interplanetary communication, etc.), detection of faint radio/microwave frequencies from astronomical bodies, detection of cosmic microwave background, and perhaps even signals from extra-terrestrial intelligent life forms as sought after by the SETI project. In some cases deliberate adulteration of signal with white noise can be useful to avoid eavesdropping. Digital cavities can significantly improve the instrumentation and reduce the cost related to high-end data acquisition/analysis systems needed in the works mentioned above.

Figure 5: Reduction of random (white) noise in a digital cavity due to waveform averaging. The signals are generated by mixing random noise five and ten times the amplitude of a sine function at 960 Hz in (a) and (b), respectively. Digitization is done at the rate of 96 kS/s. x− axis shows the index j used to denote the digitization position - one cycle is completed for j = 100; two cycles are shown in the figures. The signal to noise ratio improves in both the cases ((a) and (b)) with larger N_c. The dotted lines are fits to the cavity response using sine functions.

Another potentially important application of the digital cavity can be in high resolution spectroscopy. As shown in Equ.(5) the line-width of the cavity becomes narrower with increasing N_c, i.e. data acquisition time. This is the consequence of the fact that the precision of any interferometer depends on the number of the cycles of the sinusoidal signal that interfere. [11] In analog cavities the multi-pass within the cavity increases the number of cycles that interfere, however, the power losses in each pass sets an upper limit. Power loss in this case equates to information loss. A digital cavity is not prone to this limitation as information present in each cycle is stored digitally. Consequently, a digital cavity can have arbitrarily high precision, depending on the time over which the data is acquired. Data acquired for 1s gives a precision of about 1 Hz in the measurement of a frequency, and higher measurement time results in better precision regardless of the frequency being measured. Every digitizer, however, has the problem of electronic jitter, which introduces uncertainty in time at which digitizations happen. Jitter in digital cavity is analogous to various noise sources in an analog cavity like the thermal noise and zero point fluctuation (vacuum fluctuations). In the high end digitizers, jitter can be less than 100 fs. The jitter does not set an upper limit but increases the data acquisition time to reach the desired precision. With the currently available digitizers it would be possible to analyze the hyperfine transitions in atoms and molecules in general, and atoms used for atomic clocks in particular, with extremely high precision. As the digitization is controlled by a clock, precision measurements with a digital cavity can also be used to synchronize clocks. When a microwave of 20 GHz generated by a source controlled by a master clock is used for synchronization then the frequency measurement done by a digital cavity can be used to synchronize the clock of the digitizer to ≈ 10^{−14}s, and a day of measurement enables synchronization better than 10^{−15}s , which rivals the synchronization that can be achieved using analog techniques based on radio/microwave freqeuncies. [4] However,implementing a digital cavity with stable operation for a day or longer could be challenging.

4 Conclusion

We have presented the theoretical description of the digital cavity and derived some of its properties. Digital cavities, in general, implement the functionality of the analog cavities in time domain and eliminate problems related to power losses in the analog cavities. We have also shown examples of how digital cavities can be used in signal analysis and discussed other possible uses in signal transmission, high precision spectroscopy and precise synchronization of clocks.

Acknowledgments KK thanks Werner-Gren Foundation for the generous post-doctoral fellowship awarded to him. Financial support from the Knut and Alice Wallenberg Foundation is greatfully acknowledged.

5 Appendix A:

Bounded and unboundedness of the cavity response

To simplify the derivation of the properties of a digital cavity we represent the signal x(i · Δt), i ∈ Z as a Fourier series. Without any loss of generality, we consider a component of the series, a sine function, sin(ωt + ϕ), digitized at time intervals Δt. We use the following equation to to define a digital cavity of length n, n ∈ N^+. y(j · Δt; n) := N_c∑

k=0 sin(ω · j · Δt + ω · k · n · Δt + ϕ). (7) In (7) n·Δt = T gives the period of the cavity, thus for each j ∈ (0, 1, . . . , n− 1) the equation sums up the values at equivalent points in the successive periods for N_c times. Instead of using frequency f as done in the main text, we use angular frequency ω in the equation to reduce notations in the equations. We define ω_c = 2π/T as the fundamental frequency of the cavity. Using this definition, Equ.(7) can be written as: y(j · Δt) = N_c∑

k=0 sin ( ω · j · Δt + 2πω ω_c k + ϕ ) . (8)

We further analyse Equ.(8) in the following two cases:

First, when ω = ω_c, i.e. when the cavity is resonant with the function, the cavity simply amplifies the sine function N_c + 1 times:

y(j · Δt) = (N_c + 1) sin(ω_c · j · Δt + ϕ). (9)

Equ.(9) is true for any ω = mω_c , where m ∈ Z. Thus for all the frequencies that are integer multiple of the cavity frequency, application of the digital cavity amplifies the signal and at the same time increases the signal to noise ratio. As there are no any physical constrains that limit the amplification, it does not saturate. In other words, the amplification factor is not bounded.

Now we analyze the case when ω ≠ mω_c, i.e. when the cavity is not resonant with the function. For simplicity we analyse the case ω_c ⩽ ω ⩽ 1.5ω_c. By symmetry, the following argument also applies for the other cases. We can rewrite Equ.(8) as y(j · Δt) = N_c∑

k=0 sin ( 2πω ω_c k + ϕ_2 ) , (10)

where ϕ_2 = ω · j · Δt + ϕ. Let ω/ω_c = 1 + x with 0 ⩽ x ⩽ 0.5. Equ.(10) can be written as

y(j · Δt) = cos ϕ_2 N_c∑

k=0 sin(Ωk) + sin ϕ_2 N_c∑

k=0 cos(Ωk), with Ω = 2πx.

The sums on the right hand side have an upper bound, which can be calculated as follows. Assume N_c is very large. Take r such that Ωr ⩽ π ⩽ Ω(r+1). Then ‖ ‖ ‖ ‖ ‖ N_c∑

k=0 sin(Ωk) ‖ ‖ ‖ ‖ ⩽ r∑ k=0 sin(Ωk) Δk Δk . (11)

Let Ωk = y, then Δk =^{Δy}_Ω . Using Δk in the above ‖ ‖ ‖ ‖ N_c∑

k=0 sin(Ωk) ‖ ‖ ‖ ‖ ⩽ ∑_π y=0 sin yΔy ΩΔk ⩽ ∫_π y=0 sin ydy Ω = ω π(ω − ω_c) . Similarly ‖ ‖ ‖ ‖ N_c∑

k=0 cos(Ωk) ‖ ‖ ‖ ‖ ⩽ ω_c 2π(ω − ω_c) .

Thus for ω ≠ ω_c, F(j · Δt) is bounded by ‖F(j · Δt)‖ ⩽ ω_c 2π(ω − ω_c) (2 cos ϕ_2 + sin ϕ_2). (12)

Note that the singularity at ω_c indicates the divergence of digital cavity map at ω_c, which is also clear in Eq.(9).

The maximum value (2 cos ϕ_2 + sin ϕ_2) can have is √ 5, which gives ‖F(j · Δt)‖ ⩽ √ 5 2π ω_c ω − ω_c . (13)

Equ.(13) shows that for the case when ω ≠ ω_c, or in general when ω ≠ mω_c, the cavity response has an upper bound.

Determination of frequencies completely suppressed by a digital cavity.

If we take ω = ω_c/N_c in Equ.(10) then y(j · Δt) = N_c∑

k=0 sin ( 2πk N_c + ϕ_2 ) = 0 (14)

for all j as the summation is over a period of the sine function. Thus for a digital cavity in which the successive periods are summed N_c + 1 times there are N_c frequencies between 0 and ω_c given by ω = pω_c/(N_c + 1) where p ∈ Zandp ⩽ N_c that are completely filtered out. We define ω_c/N_c as the node distance. The nodes are present at ω = i · ω_c ± pω_c/(N_c + 1) for all i ∈ N ∧ p ∈ {1, 2, . . . , N_c}. 6 Appendix B:

Frequencies selected by digital cavity and tuning the cavity.

According to Equ.(8) for all ω = iω_c where i is an integer we have

y(j · Δt) = (N_c + 1) sin(ω · j · Δt + ϕ). (15)

Thus the cavity selects all the frequencies that are integer multiple of the fundamental frequency, in other words it selects a frequency comb with carrier offset frequency and comb tooth spacing both given by ω_c. The fundamental frequency, and thereby the comb, selected by the cavity can be changed either by changing n (number of samples digitized per unit time) or Δt (digitization interval); remember ω_c = 2π/(n · Δt). However, the definition of the digital cavity can be generalized such that carrier offset frequency and comb tooth spacing are independent. For e.g. if we define the cavity as y(j · Δt) := N_c∑

k=0 (−1)^k sin ( ω · j · Δt + 2πω ω_c k + ϕ ) (16)

then the carrier offset frequency is given by ω_c/2 while the tooth spacing is given by ω_c. Equ (16) is a special case of the general digital cavity defined as y(j · Δt; θ) := N_c∑

k=0 sin ( ω · j · Δt + 2π ( ω +^{θωc}_{2π} ω_c ) k + ϕ ) . (17)

For ω to be resonant with the cavity we need ω +^{θωc}_{2π} ω_c = 1 ⇒ θ = 2π ( 1 − ω ω_c ) (18)

The values θ can have is contrained due to the fact that data is accumulated at discrete time points and ϕ is not known in general. The general expression for the allowed values of θ in a digital cavity can be found as follows:

Equ(17) can be written as y(j·Δt) = N_c∑

k=0 sin ( ω · j · Δt + 2πω ω_c k + ϕ ) cos(θk)+ N_c∑

k=0 sin ( ω · j · Δt + 2πω ω_c k + ϕ + π 2 ) sin(θk). Using the relations ω_c = 2π n · Δt , and π 2 = ω_c · n · Δt 4 we analyze the second term

2nd term = N_c∑

k=0 sin ( ω · j · Δt + ω · n · Δt · k + n 4 · Δt · ω_c + ϕ ) .

Let ω_c = rω, then we have

2nd term = N_c∑

k=0 sin ( ω · j · Δt + ω · n · Δt · k + n 4 · Δt · r · ω + ϕ )

According to Equ.(18) we also have θ = 2π ( 1 − 1 r ) (19) Let n · r 4 = l, with l ∈ Z then r = 4l n , and θ = 2π ( 4l − n 4l ) . The frequency that resonates with the cavity is then given by ω = nω_c 4l . (20)

Finally the general expression for the cavity can be written as y(j · Δt) = N_c∑

k=0 sin(ω · j · Δt + ω · n · Δt · k + ϕ) cos ( 2π ( 4l − n 4l ) k ) + N_c∑

k=0 sin(ω · (j + l) · Δt + ω · n · Δt · k + ϕ) sin ( 2π ( 4l − n 4l ) k ) . (21)

References

[1] A. R. Leach, Molecular modelling: Principles and applications, 2nd ed., Pearson Education Limited: Harlow, 2001.

[2] M. P. Allen and D. J. Tildesley, Computer Simulation of Liquids Clarendon Press, Oxford University Press, Walton Street, Oxford OX2 6 DP, 1991.

[3] K. Karki et al., Study of structural and dynamic properties of liquid phenyltrimethoxysilane, Phys. Chem. Chem. Phys. 13 (2011) 11864.

[4] S. T. Cundiff, Femtosecond Optical Frequency Comb: Principle, Operation, and Applications Springer, Boston 2005.

[5] N. F. Scherer et al., Fluorescence-detected wave packet interferometry: Time resolved molecular spectroscopy with sequences of femtosecond phase-locked pulses, J. Chem. Phys. 95 (1991) 1487.

[6] P. F. Tekavec et al., Wave packet interferometry and quantum state reconstruction by acousto-optic phase modulation, J. Chem. Phys. 125 (2006) 194303.

[7] P. F. Tekavec et al., Fluorescence-detected two-dimensional electronic coherence spectroscopy by acousto-optic phase modulation, J. Chem. Phys. 127 (2007) 214307.

[8] K. Karki et al., Pump-probe scanning near field optical microscopy:

Sub-wavelength resolution chemical imaging and ultrafast local dynamics, Appl. Phys. Lett. 100 (2012) 153103.

[9] P. Heinonen et al., Periodic interference rejection using coherent sampling and waveform estimation, IEEE T. Circuits Syst. (1984) 438.

[10] M. Andersson et al., Flexible lock-in detection system based on synchronized computer plug-in boards applied in sensitive gas spectroscopy, Rev. Sci. Instrum. 78 (2007) 113107.

[11] G. W. Bradberry et al., Measurement of narrow linewidth with a Fabry- Perot interferometer of limited resolution Opt. Commun. 20 (1977) 307.