minη-_{max} η=ηΔ 0 1 2 3 4 5 6 7

<6.6) ηΔ (2.2<

bins N× ηΔd gap dR

-4 10

-3 10

-2 10

-1 10

1 MinBias

> 2GeV

jet1,2 T Jets, E p MP •_p MP > 4GeV

jet1,2 T Jets, E p MP •_p MP all /N gap N≡ gap R |<5.1

jet1,2 η 3.5<| CCAL gap required

CDF II Preliminary

Gap Fraction in events with a CCAL gap