arXiv:hep-ex/0012024 7 Dec 2000

Electro-Optical Detection of Charged Particles ?

Y.K. Semertzidis^a, V. Castillo^a, L. Kowalski^b, D.E. Kraus^c, R. Larsen^a, D.M. Lazarus^{a;1}, B. Magurno^{a;2}, D. Nikas^a, C. Ozben^a, T. Srinivasan-Rao^a, T. Tsang^a

aBrookhaven National Laboratory, Upton, NY 11973, U.S.A. bMontclair State University, Upper Montclair, NJ 07043 U.S.A.

cUniversity of Pittsburgh, Pittsburgh PA, 15260 U.S.A.

Abstract

We have made the first observation of a charged particle beam by means of its electro-optical effect on the polarization of laser light in a LiNbO_3 crystal. The modulation of the laser light during the passage of a pulsed electron beam was observed using a fast photodiode and a digital oscilloscope. The fastest rise time measured, 120 ps, was obtained in the single shot mode and was limited by the bandwidth of the oscilloscope and the associated electronics. This technology holds promise for detectors of greatly improved spatial and temporal resolution for single relativistic charged particles as well as particle beams.

Key words: Electro-optical devices, Charged particle detectors, Charged particle tracking, Picosecond techniques

1 Introduction

An effort has been initiated to develop an ultra-fast charged particle detector based on the birefringence, i.e. the anisotropy of the index of refraction,

⋆ Work supported in part by the U.S. Department of Energy under Contract No. DE-AC02-98CH10886 1 Corresponding author. Tel.: +1-631-344-3959;fax: +1-631-344-5954 E-mail address: lazarus@sun2.bnl.gov 2 Deceased.

Preprint submitted to Elsevier Preprint 7 December 2000 produced in an optical medium by the electric field of relativistic charged particles [1]. The anisotropy of the index of refraction implies different velocities of light propagation for orthogonal components of polarization, resulting in a phase difference between them which will produce an elliptical polarization in light that had initially been linearly polarized. The ellipticity is defined as the ratio of the semi-minor to the semi-major axis of the ellipse traced by the electric field vector projected on a plane perpendicular to the direction of propagation. The electro-optical effect in amorphous optical media is known as the Kerr effect [2] and is quadratic in the electric field E, ϕ = 2πKE^2d, where ϕ is the phase difference induced between orthogonal components of the polarized light. K is the Kerr coefficient and d is the length of the electric field region experienced by the material.

In uniaxial crystals, the induced ellipticity is linear in the E-field, and is known as the Pockels effect [3]. The difference in indices of refraction along orthogonal axes, Δn = P E where P is the Pockels constant and E is the electric field. For LiNbO_3, the Pockels constant P = 31 pm/V. The induced phase delay can be written as ϕ = 2πΔnd/λ = π(V/V_π ) with V the applied voltage and V_π the voltage required for producing a phase shift between orthogonal components of polarization equal to π radians. The maximum ellipticity of π/ √ 2 is induced when the polarization is at 45ffi with respect to the applied electric field direction.

Devices based on the Pockels effect have long been employed in the detection of fast transient electrical signals as well as for modulation of optical signals [4].

2 Apparatus

The 45 MeV kinetic energy electron beam at the Brookhaven National Laboratory Accelerator Test Facility, containing up to 1 nC in a diameter of approximately 1 mm with 10 ps duration and a repetition rate of 1.5 Hz, was scanned over a range of distances of several millimeters from the crystal.

The passage of beam bunches was detected through the effect of their electric field on the polarization of the light in a commercially available LiNbO_3 electro-optical modulator crystal. [5]. The optics setup is depicted schematically in Fig.1 The LiNbO_3 crystal was coupled to two 40 m long polarization maintaining fibers of 4 microns core diameter. The first of the fibers propagated polarized light of wavelength λ = 1.32μm from a 20 mW CW Amoco laser operating at approximately 10 mW and the second fiber returned the transmitted light to a quarter wave plate which transformed the induced ellipticity to a rotation of the initially linear polarization which had previously been nearly extinguished by the analyzer (crossed polarizer) in the absence of

Fig. 1. The experimental setup for detecting a charged particle beam. The LiNbO_3 crystal (M) was located in vacuum several mm from the beam position which could be varied over several cm. The beam direction was perpendicular to the plane of the page. The positions of the polarization maintaining fibers, polarizer (P), lenses, 1/4 wave plate (λ/4), analyzer (A), shield wall (S) and photodiode detector(PD) are schematically indicated.

the electron beam. The resulting modulation of the transmitted laser light was detected by a photodiode and pre-amplifier of 45 GHz bandwidth [6] which was followed by a 10 GHz amplifier with 32 dB gain. The output signals were digitized in a 7 GHz oscilloscope [7] and stored in memory.

The crystal modulator package had been modified to allow for the passage of the electron beam without hitting the housing. The transmitted light intensity, I, exiting the analyzer, A, is given by

I = I_0[σ^2 + (α + ϵ(t))^2] ≈ I_0[σ^2 + α^2 + 2αϵ(t)] (1)

with ϵ the induced ellipticity, and α the misalignment angle. σ^2 is the minimum possible ratio of (I/I_0) when α and ϵ are equal to zero and is defined as the extinction. A finite α can be used to linearize and amplify the effect on ϵ. It is apparent from Eq. 1, the time dependent part of the light signal can be made positive or negative depending on the sign of α relative to ϵ.

A bunched charged particle beam creates an electric field, E, at a distance r that is well approximated by Coulomb’s Law multiplied by γ, the relativistic Lorentz factor, and N_e the number of electron charges in the beam bunch for a minimum distance r_0 much greater than the dimensions of the beam bunch. E = γN_e q 4πϵ_0r^2_0 (2)

The electric field is present for Δt = r_0/γc with r_0 the effective range of the electric field, E, and c the beam velocity. Laser light travels a distance

Δl = (c/n)Δt = r_0/nγ (3)

in the crystal during the time that the electric field is present. This determines the resolving time for this technique. Since the beam was present in 10 ps bunches, the photon detection system had insufficient high frequency bandwidth to avoid signal attenuation but the high intensity, ≈ 10^{10} electrons/ bunch, provided sufficient signal amplitude for detection.

The electric field sensitivity of the LiNO_3 crystal was determined from the modulator specification provided by the manufacturer for the dependence of the phase difference on an applied high frequency voltage. For a phase difference π, the LiNbO_3 crystal had V_π = 5.7 V with an electrode separation of 15μm and a length of l = 1.5 cm. The integral ( ∫ E dl)_π = ∫ 5.7V/(15 × 10�^6 m) dl = 5700 V (4)

produces the maximum ellipticity of π/ √ 2. The integral of the electric field of the particle bunch over the crystal dimensions for a beam bunch located at the mid-plane orthogonal to the length of the crystal at a distance r_0 is ∫ Edl ≈ N_e q 4πκϵ_0nr_0 (5)

where κ is the dielectric constant and n is the index of refraction of the LiNbO_3. For r_0 = 5 mm, n = 2.2 and κ = 32 for the electric field aligned with the r_{33} axis, ∫ Edl = 4.1 × 10�^9N_e V which with Equation 4 yields an ellipticity ϵ = ∫ Edl ( ∫ Edl)_π × π/ √ 2 = 7.2 × 10�^{13}N_e (6)

The signal to noise ratio for a measurement of this type that is photon statistics limited is given by SNR = ϵ √ P T q_p 2hν (7)

where P is the laser power, T the time resolution or inverse of the detection system bandwidth, q_p the quantum efficiency of the photodiode, and hν the laser photon energy. Excellent time resolution results in enhanced sensitivity,

Fig. 2. The polarization dependent signal (solid line). The electron beam was

ß 0.5 cm from the crystal. The polarization independent signal is indicated by

the dashed line.

which can be essential for the detection of extremely short pulses, but it will also increase white noise acceptance due to the increased bandwidth.

3 Experimental Results

Measurements were made in the single shot mode using the 7 GHz oscilloscope. The extinction was approximately 2 × 10�^3. With P = 10 mW, T = 100 ps, q_p = 0.8 and hν = 0.9 eV, Eqs.6 and 7 determine the required number of electrons in the beam for SNR = 1, N_e ≈ 8×10^8 for detection of a single beam bunch. However, the 7 GHz bandwidth limits the sensitivity to the inherently much faster signal by as much as factor of five implying ≈ 4 × 10^9 singly charged particles are required for detection of a single ATF beam bunch. The ATF beam of N_e = 6.3 × 10^9 per bunch was sufficient to generate a detectable modulation.

The polarization dependent signal is displayed in Fig. 2 (solid curve). Changing the sign of α (see Eq. 1) caused the sign of the signal to change whereas the amplitude was unaffected. The maximum modulation of the light intensity was ≈ 9% of its DC level.

A negative signal due to the attenuation of light was observed when the LiNO_3 crystal intercepted the beam. It was found to be polarization independent and has a significantly longer decay time constant than the polarization dependent signal. A similar effect was found in poled quartz fibers and polarization maintaining fibers.

4 Discussion

Although it presently appears possible to construct a beam profile detector with excellent time resolution based on parallel rows of LiNbO_3 crystals , a more formidable challenge would be to achieve single particle detection with this technology. With a high power pulsed laser of 10^9 W, i.e. 10 mJ for 10 ps and a transient digitizer of greater bandwidth, e.g. 60 GHz, a detector constructed of parallel rows of electro-optical crystals with a separation of 100μm and therefore an effective average distance, r_0 ≈ 25μm between a single charged particle trajectory and the nearest fiber can be assumed. Equations 5 and 6 would then give an ellipticity ϵ = 1.4 × 10�^{10} and Equation 7 gives SNR ≈ 2.3 × 10�^2 for single particle detection with LiNiO_3.

In addition, use of a high power pulsed laser would preclude the detection of randomly occurring events because of the inability to trigger the laser. However, this would be ameliorated somewhat at colliding beams machines where the beams are tightly bunched and interact periodically to maximize the luminosity.

The small size and high cost of the LiNbO_3 crystals has prompted a search for materials of larger electro-optical coefficients and lower dielectric constants. We have measured the Kerr coefficients of optical fibers and quartz rods to be 10�^4 − 10�^3 pm/V^2. Organic liquids such as nitrobenzene have relatively large Kerr coefficients and could be used in hollow glass fibers of micron dimensions. Although these could lead to inexpensive devices, the Kerr coefficients are less than 2.5 pm/V^2 which is far too small for sensitivity to singly charged particles.

Electrically poled optical fibers have been shown to produce relatively large electro-optical effects [8]. At sensitivities as high as 0.1 nm/V^2 they may be adequate for charged particle beam diagnostics but it is unlikely that it will be sufficiently sensitive for single particle detection.

DAST (4-dimethylamino-N-methyl-4-stilbazolium tosylate) crystals [9] have been found to have large electro-optic coefficients, from 47 ± 8 pm/V at λ = 1535 nm to 92 ± 9 pm/V at λ = 720 nm as well as a small dielectric constant, κ = 5.2 compared to 30.8 pm/V and κ = 32 for LiNbO_3. This implies a factor of 20 greater sensitivity than LiNbO_3. If DAST or yet to be developed electrooptical materials can yield adequate sensitivity for single particle detection, a new generation of ultrafast fine grained charged particle detectors may be at hand.

5 Acknowledgements

We wish to acknowledge the support and encouragement of Xiejie Wang, Ilan Ben-Zvi, Vitaly Yakimenko, John Miller, Howard Gordon, Mike Murtagh and Tom Kirk. The efforts of Victor Usack and the contributions of our late colleague Ben Magurno were essential to our progress.

References

[1] Y.K. Semertzidis, XXVII International Conference on High Energy Physics gls0918 (1994)(Unpublished).

[2] J. Kerr, Phi. Mag. 50 (1875) 337, 446

[3] F. Pockels, Abhandl. Ges. Göttingen Math.-Phizik. Kl. 39 (1894) 1. A. Yariv, Quantum Electronics, Wiley, New York, 3rd ed. 1989.

[4] W. Willis, Proc. ECFA/INFN Workshop. CERN 85/07 (1985) 166 J.A.

Valdmannis, G. Mourou and C.W. Gabel, IEEE J. Quantum Electronics QE- 19 (1983) 664. C. Bamber et al, Nucl. Instrum. Methods Phys. Res. Sect. A 327 (1993)227. T. Tsang and V. Radeka, Rev. Sci. Instrum. 66(7) (1995) 3844

[5] Uniphase Telecommunications Products, 1289 Blue Hills Ave., Bloomfield, CT 06002.

[6] Type 1011 pre-amplifier from New Focus, Inc., 2630 Walsh Ave., Santa Clara, CA 95051. The conversion gain of the detector is 10 V/W, with a rise time of 9 ps.

[7] The digitizing oscilloscope used was a Tektronix SDC 5000 of 7 GHz bandwidth.

[8] X.C. Long and S.R.J. Brueck, IEEE Photonic Technol. Lett. 9 (1997) 767. David J. Welker et al., Opt. Lett. 23(23) (1998) 1826

[9] F. Pan et al., Appl. Phys. Lett. 69(1) (1996) 13