arXiv:nucl-ex/0602001 v1 2 Feb 2006

Tracking in Antiproton Annihilation Experiments

Olaf N. Hartmann^a

aLaboratori Nazionali di Frascati dell’INFN Via E. Fermi,40, 00044 Frascati (RM), Italy

Abstract

A major ingredient of the planned new accelerator complex FAIR, to be constructed at the GSI, Darmstadt, Germany, is the availability of antiproton beams with high quality and intensity. Among the experiments which will make use of this opportunity is PANDA, a dedicated experiment to study antiproton annihilations on nucleons and nuclei. This article gives an overview on the foreseen techniques to perform charged particle tracking in the high rate environment of this experiment.

Key words:

PACS: 13.75.-n, 13.75.Cs, 13.75.Ev, 13.20.-v, 25.43.+t

1 Introduction

With the future FAIR [1] facility at the GSI [2] in Darmstadt, Germany, beams of antiprotons will become available. After production using a primary proton beam, collecting and cooling, the antiprotons will be delivered to a dedicated synchrotron/storage ring (named HESR), where they will be stored, accelerated/decelerated to the desired energy, cooled and used for experiments with an internal target (p, A). The momentum range of the p beam will be between 1.5 and 15 GeV/c, i.e. the maximum pp center-of-mass energy will be 5.5 GeV. The design luminosity is 2·10^{32} cm^{−2}s^{−1}, and a momentum spread of δp/p ≈ 10^{−4} is envisaged. With a somewhat relaxed demand in luminosity, δp/p ≈ 10^{−5} should be achievable. These parameters translate into an annihilation rate of about 10^7 s^{−1} = 10 MHz, thus despite having a moderate multiplicity per event the experiment has to deal with high rates.

Preprint submitted to Elsevier Science 2 February 2006

2 Experimental Evironment

The antiproton annihilations occuring on the internal target are to be studied by the PANDA [3] detector. PANDA is a fixed target experiment which consists of a target spectrometer surrounding the interaction point and a forward spectrometer to measure down to 0^∘ in polar angle. Figure 1 shows the schematic view (from the top) of the whole setup. The figure is taken from [4]. Further details of the experimental setup can be found in [4].

Fig. 1. Top view of the PANDA setup.

The requirements to the charged particle tracking systems are: a solid angle coverage of nearly 4π, the capability to resolve multiple tracks, good spatial resolution for secondary vertices, high momentum resolution O(1%) in a range from MeV/c to several GeV/c, minimal material budget, high rate capability (the occupancy reaches values of ≈ 3 · 10^4 cm^{−2}s^{−1} in the forward region) and robustness against ageing effects. Finally it operates in a magnetic field. As indicated in Fig. 1, the experiment applies a solenoid field (2 T) for the target spectrometer and a dipole field (2 Tm) for the forward part. The components of the tracking system are:

• a microvertex detector (MVD) close to the interaction point (IP), using silicon pixel/silicon strip detectors • a central tracker surrounding the MVD, made from straw tubes, or, as an alternative under study, using a time projection chamber • drift chambers in the target and the forward spectrometer for the particles emitted under small polar angles

In the following, this article focuses on the straw tube central tracker; more information and details about the other tracking devices can be found in [4].

3 The central tracker

The straw tube tracker (STT) is a cylindrical object consisting out of several double layers of straw tubes oriented along the beam axis. It should cover the radial space from 15 to 42 cm with respect to the beam axis. In the left part of Fig. 2, a possible arrangement using 11 double layers is shown; the beam pipe in the center and the perpendicular target pipe are shown as well. The tubes have a diameter of 6 mm for the inner layers and 8 mm for the outer layers; 20 μm ∅ W-Re is used for the anode wires, and a mylar/kapton film with Al coating for the tubes. The counting gas has been chosen to be a mixture of 90% Ar and 10% CO_2, at normal or slight overpressure. In such a configuration, one tube amounts to 0.05% X/X_0 material budget, and the full device to approximately 1% (excluding cables and support structures at the downstream/upstream end).

Fig. 2. Left: The central tracker made from straw tubes. The support structures are not shown. Right: Relative comparison of the resolution as a function of the number of double layers for various particle momenta.

The basic arrangement in double layers is needed to resolve the left-right ambiguity of the passage of a charged particle with respect to the wire. In the right part of Fig. 2 a relative comparison of the resolution as a function of the number of double layers is shown for different momenta of the traversing particles, which for this simulation are μ^− emitted under an angle of 45^∘ from the nominal interaction point. The resolution has been extracted from the width of a gaussian fit to the appropriate 1/p distributions [5]. As one can see, with a number of 11(±1) double layers the requirements for low and high momentum particles can be satisfied, adding more double layers does not improve the overall resolution. Together with an additional information from the vertex detector, the momentum resolution reaches a level of 1.5 to 2% over the whole quoted momentum range.

Fig. 3. Left: Simulation of a physics channel using STT. Right: Photograph of a straw tube prototype prepared at the LNF.

In the left part of Fig. 3 the result of a physics channel using a full scale Monte Carlo [4] with the STT for particle tracking is shown as an example: the Ψ(3770) resonance, formed in a pp annihilation, decays into a DD pair. The channel D^± →K^∓π^±π^± is reconstructed. Here, the invariant mass distribution is plotted; the Ψ(3770) can be reconstructed with a resolution of σ_Ψ ≈ 10 MeV/c^2 and a reconstruction efficiency of ≈4%.

Concerning the gas mixture, He and Ar based mixtures have been studied in a simulation [4,7]. Finally, the above mentioned Ar:CO_2 9:1 mixture has been chosen since it has a high number of primary ionisations per track length, and thus gives a better efficiency and spatial resolution. The efficiency, measured with a 10 mm ∅ straw [6] is ≈99% over the major part of the tube; very close to the tube wall (last 0.25 mm) it drops to ≈75% due to the low number of primary ionisations along the short track piece. The drift time is smaller than 100 ns and thus matches the expected interaction rates. The spatial resolution of such a detector is < 150μm in rφ. Since the tubes have the readout only on one side, the z coordinate instead could be obtained by using stereo tubes, i.e. rotating several double layers by a small so-called skew angle of 2-3^∘ to resolve the ambiguities. With this method in principle a z resolution of several mm can be achieved. Under investigation is the possibility to connect two neighbouring tubes, thus allowing a two-side readout, and to obtain the z coordinate by charge division. As discussed in [7], one could expect a resolution of 7 to 15 mm. Nevertheless, at present only a resolution in the order of > 2 cm could be reached in tests with a radioactive source, further improvement is needed to make this method competitive with the skewed tubes. The geometry and the mechanical mounting of the STT is fairly complicated due to the presence of beam- and target pipe and the lack of overall space (see Fig. 2, right, and Fig. 1) inside the coil of the solenoid. These questions are currently under study. Finally, the right part of Fig. 3 shows a photograph of a straw tube prototype constructed at the INFN Frascati laboratories to be used for further R&D.

4 Acknowledgments

I acknowledge the support of the European Community-Research Infrastructure Activity under the FP6 “Structuring the European Research Area” programme (HadronPhysics, contract number RII3-CT-2004-506078).

References

[1] Facility for Antiproton and Ion Research, http://www.gsi.de/fair

[2] Gesellschaft für Schwerionenforschung mbH, http://www.gsi.de/

[3] P Annihilation at Darmstadt, http://www.gsi.de/panda

[4] Strong Interaction Studies with Antiprotons, Technical Progress Report for PANDA, Darmstadt, 01/2005

[5] L. Lavezzi, private communication

[6] P. Wintz et al., AIP conference proceedings, 698 (2004) 789

[7] A. Sokolov, Dissertation, University of Giessen, 2005