arXiv:physics/0509164 v1 20 Sep 2005

DESY 05-164 September 2005

Properties of the odd harmonics of the radiation from SASE FEL with a planar undulator

E.L. Saldin, E.A. Schneidmiller, and M.V. Yurkov

Deutsches Elektronen-Synchrotron (DESY), Hamburg, Germany

Abstract

Recent theoretical and experimental studies have shown that Self-Amplified Spontaneous Emission Free Electron Laser (SASE FEL) with a planar undulator holds a potential for generation of relatively strong coherent radiation at the third harmonic of the fundamental frequency. Here we present detailed study of the nonlinear harmonic generation in the SASE FEL obtained with time-dependent FEL simulation code. Using similarity techniques we present universal dependencies for temporal, spectral, and statistical properties of the odd harmonics of the radiation from SASE FEL. In particular, we derived universal formulae for radiation power of the odd harmonics at saturation. It was also found that coherence time at saturation falls inversely proportional to harmonic number, and relative spectrum bandwidth remains constant with harmonic number.

Preprint submitted to Optics Communications

1 Introduction

Radiation of the electron beam in the planar undulator contains rich harmonic spectrum. This referes to both, incoherent and coherent radiation as well. During last years a significant efforts of researchers have been devoted for studying the process of the higher harmonic generation in the high-gain free electron lasers [1]-[11]. Such an interest has been mainly driven by practical needs for prediction of the properties of X-ray free electron lasers. A fraction of a higher harmonic content is very important for users planning experiments at X-ray FEL facility. On the one hand, higher harmonics constitute rather harmful background for some classes of experiments. On the other hand, higher harmonic radiation can significantly extend operating band of the user facility. In both cases it is highly desirable to know properties of the hiher harmonic radiation. Analytical techniques have been used to predict properties of the higher harmonics for FEL amplifier operating in the linear mode of operation [8,9]. However, the most fraction of the radiation power is produced in the nonlinear regime, and a set of assumptions needs to be accepted in order to estimate saturation power of higher harmonics on the base of extrapolation of analytical results. As for statistical properties, they could not be extrapolated from linear theory at all. A lot of studies has been performed with numerical simulation codes. These studies developed in two directions. The first direction is investigations of higher harmonic phenomena by means of steady-state codes [4,5,6,7]. Despite the results of these studies are applicable to externally seeded FEL amplifiers, it is relevant to appreciate that they gave the first predictions for high radiation power in higher harmonics of SASE FEL. Another direction was an extraction of time structure for the beam bunching from time-dependent simulation code with subsequent use of analytical formulae of the linear theory [8]. Giving an estimate for the power, such an approach does not allow to describe statistical properties of the output radiation.

In this paper we perform comprehensive study of the statistical properties of the odd harmonic radiation from SASE FEL. The study is performed in the framework of one-dimensional model with time-dependent simulation code FAST [12,14] upgraded for simulation of higher harmonic generation. We restrict our study with odd harmonics produced in the SASE FEL. We omit from consideration an effect of self-consistent amplification of the higher harmonics. In other words, we solve only electrodynamic problem assuming that particle motion is governed by the fundamental harmonic. The latter approximation is valid when power in higher harmonics is much less than in the fundamental. This does not limit practical applicability of the results: it has been shown in earlier papers that the growth rate of higher harmonics is too small to produce visible increase of the coherent amplification above shot noise in X-ray FELs [8]. Under this approximation and using similarity techniques we derive universal relations describing general properties of the odd harmonics in the

SASE FEL: power, statistical and spectral properties. The results are illustrated for the 3rd and 5th harmonic having practical importance for X-ray FELs.

2 Basic relations

The one-dimensional model describes the amplification of the plane electromagnetic wave by the electron beam in the undulator. When space charge and energy spread effects can be neglected, operation of an FEL amplifier is described in terms of the gain parameter Γ = [πj_0K^2_1 /(I_Aλ_wγ^3)]^{1/3}, efficiency parameter ρ = λ_w Γ/(4π), and detuning parameter Ĉ = [2π/λ_w − ω(1 + K^2/2)/(2cγ^2 )]/Γ (see,e.g. [13,14]). Here λ_w is undulator period, K = eλ_wH_w /2πmc^2 is undulator parameter, γ is relativistic factor, H_w is undulator field, j_0 is the beam current density, (−e) and m are charge and mass of electron, I_A = mc^3/e ≃ 17 kA, and ω is frequency of electromagnetic wave. Coupling factor K_h is given by

K_h = K(−1)^{(h−1)/2}[J_{(h−1)/2}(Q) − J_{(h+1)/2}(Q)] , (1)

Q = K^2/[2(1 + K^2)], and K is rms undulator parameter. When describing start-up from shot noise, one more parameters of the theory appears – number of particles in coherence volume, N_c = I/(eρω), where I is beam current.

We do not present here general technical details of the time dependent simulations, they have described previously in details [12,14]. The only add-on to these description is particle loading tool, but it is similar to that described in other papers (see, e.g. [15] and references therein). We note only that under accepted approximation (particle’s dynamics is governed by the fundamental harmonic) we can simply calculate odd harmonics from particle distribution, and amplitude of the electric field scales as

E(z, t) ∝ K_h z∫ 0 a_h(z^′, t − z^′/c)dz^′ , (2)

where a_h is h-th harmonic of the beam bunching. Thus, we find that coupling factor K_h, and time-dependent integral of the beam bunching become to be factorized. This allows us to extract universal ratio of the power of higher harmonics to the power of fundamental harmonic.

3 Statistical properties of the odd harmonics of the radiation from SASE FEL

In this section we present the results of numerical studies of the operation of the SASE FEL in the linear and nonlinear regimes. In the framework of the accepted model, the input parameter of the system is the number of cooperating electrons N_c. Most of the statistical characteristics of the SASE FEL process are functions of N_c only in the fixed z coordinate. A typical range of the values of N_c is 10^6 − 10^9 for the SASE FELs of wavelength range from X-ray up to infrared. The numerical results, presented in this section, are calculated for the value N_c = 3×10^7 which is typical for a VUV FEL. It is worth mentioning that the dependence of the output parameters of the SASE FEL on the value of N_c is rather weak, in fact logarithmic. Therefore, the obtained results are pretty general and can be used for the estimation of the parameters of actual devices with sufficient accuracy.

3.1 Temporal characteristics

Figure 1 presents a typical time structure of the 1st and the 3rd harmonic of the radiation from a SASE FEL at different undulator length ẑ = Γz = 10−13. Normalized power of h-th harmonic is defined as η̂_h = W_h × (K_1/K_h)^2/(ρW_b). Longitudinal coordinate along the pulse is ŝ = ρω_0(z/v̄_z − t). The head of the pulse is located in the positive direction of ŝ. A plot for the averaged power of the 1st harmonic is shown in Fig 2 with a solid line. It is seen that saturation is achieved at the undulator ẑ = 13. Saturation length is well described in terms of the number of cooperating electrons N_c [14,16]:

ẑ_{sat} ≃ 3 + 1 √ 3 ln N_c . (3)

The normalized efficiency at saturation, η̂_{sat} = W_{sat}/(ρW_b) ≃ 1.08, is almost independent of the value of N_c. Dashed and dotted lines show a normalized power ratio, η̂_h/η̂_1 = (W_h/W_1) × (K_1/K_h )^2, for the 3rd and the 5th harmonic. One can notice that power of the higher harmonics becomes to be above the shot noise level only in the end of linear regime. This becomes clear if one takes into account that the shot noise level of the beam bunching is about 1/ √ N_c. We consider an example typical for VUV FEL with N_c = 3 × 10^7 which corresponds to the shot noise beam bunching a ≃ 2 × 10^{−4}. When FEL amplifier operates in the linear regime, odd harmonics grow as a^h_1 , and we expect from this simple physical estimation that coherent contribution into higher harmonics can exceed the shot noise level only for the values of the beam bunching at the fundamental harmonic a_1 ≳ 0.1, i.e. in the end

Fig. 1. Normalized power in the radiation pulse versus ŝ = ρω_0(z/v̄_z −t) at different lengths of the FEL amplifier ẑ = 10 − 13. Left and right columns correspond to the fundamental and 3rd harmonic, respectively

of the linear regime. Note that shot noise level becomes to be higher when approaching to X-ray region.

Fig. 2. Normalized averaged power of a fundamental harmonic of SASE FEL, η̂_1 = P_1/(ρP_{beam}), as a function of a normalized undulator length (solid line). Dashed and dotted lines show a normalized power ratio, η̂_h/η̂_1 = (W_h/W_1) × (K_1/K_h)^2, for the 3rd and 5th harmonic

Fig. 3. Ratio of coupling factors, (K_h/K_1)^2, for the 3rd (solid line) and the 5th (dashed line) harmonics with respect the fundamental harmonic versus rms value of undulator parameter K_{rms}

The plots presented in Fig. 1 allows to trace the evolution of the 3rd harmonic power from ẑ = 10 (when it just started to exceed shot noise level) up to saturation point ẑ = 13. When the beam bunching at the fundamental harmonic is governed by a sine function (i.e. SASE FEL operates in the linear regime), we

Fig. 4. Normalized power growth rate for the 1st, 3rd, and 5th harmonic (solid, dashed, and dotted line, respectively)

occur well-known mechanism of the higher harmonic generation, i.e. a_h ∝ a^h_1 , and spikes of the 3rd harmonic radiation become rather pronouncing. At this stage, for instance, the growth rate of the higher harmonics should be proportional to the harmonic number [4,5,8]. The plot of the power growth rate for the 1st, 3rd, and 5th harmonic is shown in Fig. 4. One can see from this plot that in practical situation for SASE FEL the growth rates of higher harmonics are visibly less than those given by prediction of the linear theory. This is due to the fact that the value of a_1 ≃ 0.1 can not be considered as a linear stage, and the beam density modulation is not a sine-like due to nonlinear effects. The noise nature of the SASE FEL makes a big difference in the behavior of the growth rates with respect to preidctions given in the framework of steady-state simulations [4,5]. Analyzing the plot for the power growth rate we can state that in practical situation predictions of the steady-state theory are valid only for the 3rd harmonic, but only on a short piece of undulator close to saturation, of about one gain length. Quantitative analysis of this stage of amplification shows that a prediction for the relation between averaged values of the beam bunching at the third harmonic, < |a_3|^2 >= 6 < |a_1|^2 >^3, holds approximately, and is strongly violated for higher harmonics, because of strong contribution of the shot noise. This feature of the SASE FEL has been highlighted qualitatively in early papers [8] with analysis of simulation results obtained with code GINGER [3]. Here we just presented more quantitative study.

The plots in Fig. 2 present a general result for a ratio of the power in the higher harmonics with respect to the fundamental one. For the saturation we

Fig. 5. Normalized power ratio at saturation, (W_h/W_1) × (K_1/K_h)^2, for the 3rd (solid line) and 5th (dashed line) harmonic as a function of energy spread parameter Λ̂2_T. SASE FEL opeartes at saturation

find a universal dependency: ⟨W_3⟩ ⟨W_1⟩ |_{sat} = 0.094 ×

K^2_3 K^2_1 , ⟨W_5⟩ ⟨W_1⟩ |_{sat} = 0.03 ×

K^2_5 K^2_1

. (4)

Universal functions for the ratio (K_h/K_1)^2 are plotted in Fig. 3. Asimptotic values for large value of undulator parameter are: (K_3/K_1)^2 ≃ 0.22, and (K_5/K_1)^2 ≃ 0.11. Thus, we can state that contribution of the 3rd harmonic into the total radiation power of SASE FEL at saturation could not exceed a level of 2%. Thus, its influence on the beam dynamics should be small. This result justifies a basic assumption used for derivation of a universal relation (4). A contribution of the 5th harmonic into the total power at saturation could not exceed the value of 0.3%.

Another important topic is an impact of the electron beam quality on the nonlinear harmonic generation process. In the framework of the one-dimensional theory this effect is described with the energy spread parameter Λ̂^2_T [14]:

Λ̂^2_T = ⟨(ΔE)^2⟩ ρ^2E^2_0 ,

where ⟨(ΔE)^2⟩ is the rms energy spread. Thus, result given by (4) is generalized to the case of finite energy spread with the plot presented in Fig. 5. We see that the energy spread in the electron beam suppresses power of the higher harmonics. Within practical range of Λ̂^2_T this suppression can be about a factor of 3 for the 3rd harmonic, and about an order of magnitude for the 5th harmonic. For practical estimations one should use an effective value of the energy spread describing contribution of the energy spread and emiitance to the longitudinal velocity spread [14]:

⟨(ΔE)^2⟩_{eff} E^2_0 = ⟨(ΔE)^2⟩ E^2_0 + 2γ^4_z ϵ^2 β^2 ,

where γ_z is longitudinal relativistic factor, ϵ is beam emittance, and β is focusing beta-function. The plot in Fig. 5 covers practical range of parameters fo X-ray FELs. The saturation length at Λ̂^2_T = 0.5 is increased by a factor of 1.5 with respect to the ”cold” beam case Λ̂^2_T = 0.

3.2 Probability distributions

The next step of our study is the behavior of the probability distribution of the instantaneous power. In Fig. 6 we show the normalized rms deviation of the instantaneous radiation power, σ_w = ⟨(W − ⟨W ⟩)^2⟩^{1/2}/⟨W ⟩, as a function of the undulator length. We see that at the initial stage of SASE FEL operation rms deviation of the instantaneous power is equal to one for all harmonics. This is a consequence of start-up from the shot noise in the electron beam: sta-

Fig. 6. Normalized rms deviation of the fluctuations of the instanteneous radiation power as a function of the normalized undulator length. Solid, dashed, and dotted lines correspond to the fundamental, 3rd, and 5th harmonic, respectively tistical properties of the undulator radiation and of the radiation from SASE FEL operating in the linear regime are governed by Gaussian statistics [14,16]. One of the important features of the Gaussian statistics is that the normalized rms deviation of the instantaneous radiation power is equal to the unity. For the fundamental harmonic statistics of the radiation becomes to be non- Gaussian when the amplification process enters non-linear mode [14,16]. For the higher harmonics non-Gaussian statistics takes place when the nonlinear harmonic generation starts to dominate above incoherent radiation (at ẑ ≳ 8 in the present numerical example). Analytical theory of nonlinear harmonic generation [8] predicts the value of σ_w ≃ 4 for the third harmonic. Analysis of the relevant curve in Fig. 6 shows that this prediction holds approximately in a short piece of the undulator length only. As we explained above, this is due to the fact that nonlinear harmonic generation starts to dominate above incoherent radiation only at the values of the beam bunching at the fundamental harmonic a_1 ∼ 0.1. However, at such a value of the beam bunching the modulation of the beam density already deviates from a sin-like shape due to nonlinear effects.

Probability density distributions for the instantaneous power of the fundamental and the 3rd harmonic are presented in Fig. 7. SASE radiation is a stochastic object and at a given time it is impossible to predict the amount of energy which flows to a detector. The initial modulation of the electron beam is defined by the shot noise and has a white spectrum. The high-gain FEL amplifier cuts and amplifies only a narrow frequency band of the initial spectrum Δω/ω ≪ 1. In the time domain, the temporal structure of the fundamental harmonic radiation is chaotic with many random spikes, with a typical duration given by the inverse width of the spectrum envelope. Even without performing numerical simulations, we can describe some general properties of the fundamental harmonic of the radiation from the SASE FEL operating in the linear regime. Indeed, in this case we deal with Gaussian statistics. As a result, the probability distribution of the instantaneous radiation intensity W should be the negative exponential probability density distribution [14,16]:

p(W ) = 1 ⟨W ⟩ exp ( − W ⟨W ⟩ ) . (5)

Here one should realize clearly that the notion of instantaneous intensity refers to a certain moment in time, and that the analysis must be performed over an ensemble of pulses. Also, the energy in the radiation pulse E should fluctuate in accordance with the gamma distribution [14,16]:

p(E) = M^M Γ(M) ( E ⟨E⟩ )_{M −1} 1 ⟨E⟩ exp ( −M E ⟨E⟩ ) , (6)

Fig. 7. Probability distribution of instanteneous radiation power at different lengths of the FEL amplifier ẑ = 10 − 13. Left and right columns correspond to the fundamental and 3rd harmonic, respectively. Solid line shows probability density function (7) where Γ(M) is the gamma function of argument M, and 1/M = ⟨(E − ⟨E⟩)^2⟩/⟨E⟩^2 is the normalized dispersion of the energy distribution. These properties are well known in statistical optics as properties of completely chaotic polarized radiation [18].

The statistics of the high-harmonic radiation from the SASE FEL changes significantly with respect to the fundamental harmonic (e.g., with respect to Gaussian statistics). It is interesting in our case to be able to determine the probability density function of instantaneous intensity of SASE radiation after it has been subjected to nonlinear transformation. We know the probability density function p(W ) = ⟨W ⟩^{−1} exp(−W/⟨W ⟩) of the fundamental intensity W , and W is subjected to a transformation z = (W )^n. The problem is then to find the probability density function p(z). It can be readily shown that this probabilty distribution is [17]: p(z) = z n⟨W ⟩ z^{(1−n)/n} exp(−z^{1/n}/⟨W ⟩) . (7)

Using this distribution we get the expression for the mean value: ⟨z⟩ = n!⟨W ⟩^n. Thus, the nth-harmonic radiation for the SASE FEL has an intensity level roughly n! times larger than the corresponding steady-state case, but with more shot-to-shot fluctuations compared to the fundamental [8]. Nontrivial behavior of the intensity of the high harmonic reflects the complicated nonlinear transformation of the fundamental harmonic statistics. One can see that Gaussian statistics is no longer valid. Upper plots in Fig. 7 give an illustration to these consideration. Despite in practical example we do not have pure linear amplification regime, the probability density functions for the instanteneous power follow rather well prediction (7).

Analysis of the probability distributions in Fig. 7 shows that in the nonlinear regime, near the saturation point, the distributions change significantly with respect to the linear regime for both, the fundamental and the 3rd harmonic. An important message is that at the saturation point the 3rd harmonic radiation exhibits much more noisy behaviour (nearly negative exponential) while stabilization of the fluctuations of the fundamental harmonics takes place.

3.3 Correlation functions

The first and the second order time correlation functions are defined follows:

g_1(t − t^′) = ⟨Ẽ(t)Ẽ^∗(t^′)⟩ [ ⟨|Ẽ(t)|^2⟩⟨|Ẽ(t^′)|^2⟩ ]_{1/2} ,

g_2(t − t^′) = ⟨|Ẽ(t)|^2|Ẽ(t^′)|^2⟩ ⟨|Ẽ(t)|^2⟩⟨|Ẽ(t^′)|^2⟩ . (8)

In Fig. 8 we show the evolution of the time correlation functions of first and second order. At each normalized position along the undulator, ẑ, they are

Fig. 8. First (left column) and second (right column) order correlation function at different lengths of the FEL amplifier ẑ = 10 − 13. Solid, dashed, and dotted lines correspond to the fundamental, 3rd and 5th harmonic, respectively

plotted versus the normalized variable τ̂ = ρω_0(t − t^′). Upper plot in Fig. 8 corresponds to the linear stage of SASE FEL operation. In the case of the fundamental harmonice we deal with a Gaussian random process and the relation between the correlation functions holds for g_2(t − t^′) = 1 + |g_1(t − t^′)|^2. This feature does not hold place for figher harmonics. The nontrivial behavior of the correlation functions reflects the complicated nonlinear evolution of the SASE FEL process. The second-order correlation function of zero argument,

Fig. 9. Normalized coherence time of a SASE FEL as a function of normalized undulator length. Solid, dashed, and dotted lines correspond to the fundamental, 3rd, and 5th harmonic, respectively

g_2(0), takes values smaller or larger than two, but always larger than unity. Note that there is a simple relation between g_2(0) and the normalized rms power deviation: g_2(0) = 1 + σ^2_w (see Fig. 6). It is a well-known result of statistical optics that the cases of g_2(0) = 1 and g_2(0) = 2 correspond to stabilized single-mode laser radiation and to completely chaotic radiation from a thermal source, respectively. The values of g_2(0) between 1 and 2 belong to some intermediate situation. In classical optics, a radiation source with g_2(0) < 1 cannot exist but the case of g_2(0) > 2 is possible. As one can see from Fig. 8, the latter phenomenon (known as superbunching) occurs for higher harmonics of SASE FEL, or for fundamental one when the SASE FEL operating in the nonlinear regime.

In Fig. 9 we present the dependence on the undulator length of the normalized coherence time τ̂_c = ρω_0τ_c, where τ_c is

τ_c = ∞∫ −∞ |g_1(τ )|^2 d τ . (9)

For the fundamental harmonic the coherence time achieves its maximal value near the saturation point and then decreases drastically. The maximal value of τ̂_c depends on the saturation length and, therefore, on the value of the parameter N_c. With logarithmic accuracy we haave the following expression for the coherence time of the fundamental harmonic:

(τ̂_c)_{max} ≃ √ π ln N_c 18 .

One can find from Fig. 8 that coherence time at saturation for higher harmonics approximately falls inversely proprtional to the harmonic number h.

3.3.1 Spectral Characteristics

When comparing radiation spectra, it is convenient to use the normalized spectral density, h(Ĉ), defined as ∞∫ −∞ d Ĉh(Ĉ) = 1 .

The frequency deviation, Δω, from the nominal value of ω_h can be recalculated as Δω = −2ρω_hĈ. Since we consider the model of a long rectangular bunch, the function h(Ĉ) can be treated as the normalized spectral density of both

Fig. 10. Normalized spectrum at different length of the undulator: ẑ = 10−13. Solid, dashed, and dotted lines correspond to the fundamental, 3rd and 5th harmonic, respectively the radiation energy and the power.

Normalized envelope of the radiation spectrum and the first order time correlation function are connected by the relation [18]:

G(Δω) = 1 2π ∞∫ −∞ dτ g_1(τ ) exp(−iΔωτ ) . (10)

The temporal structures of the radiation pulses (see Fig. 1) are used for calculating the first order time correlation function (see Fig 8). Then the radiation spectra are reconstructed by Fourier transformation of the first order time correlation function. Figure 10 shows evolution of the radiation spectra of the SASE FEL radiation from the end of the linear regime to saturation. Note that spectrum width of the higher harmonics from SASE FEL differs significantly from that of incoherent radiation. For the case of incoherent radiation relative spectrum width, Δω/ω_h scales inversely proportional to the harmonic number h [19]. One can see that situation changes dramatically for the case when nonlenear harmonic genaration process starts to be dominant. At saturation we find that relative spectrum bandwidth becomes to be nearly the same for all odd harmonics.

4 Summary

In this paper we performed detailed study of the properties of the odd harmonic of the radiation from SASE FEL. Universal formulae for contribution of the higher odd harmonics to the FEL power for SASE FEL operating at saturation are obtained. In the case of cold electron beam these contributions are functions of the undulator parameter K only. General statistical properties of the odd harmonics of the SASE FEL operating in saturation are as follows. Power of higher harmonics is subjected to larger fluctuations than that of the fundamental one. Probability distributions of the instantaneous power of higher harmonics is close to the negative exponential distribution. The coherence time at saturation falls inversely proportional to harmonic number, and relative spectrum bandwidth remains constant with harmonic number.

References

[1] M. Schmitt and C. Elliot, Phys. Rev. A, 34(1986)6.

[2] R. Bonifacio, L. De Salvo, and P. Pierini, Nucl. Instr. Meth. A293(1990)627. [3] W.M. Fawley, Proc. IEEE Part. Acc. Conf., 1995, p.219. [4] H. Freund, S. Biedron and S. Milton, Nucl. Instr. Meth. A 445(2000)53. [5] H. Freund, S. Biedron and S. Milton, IEEE J. Quant. Electr. 36(2000)275. [6] S. Biedron et al., Nucl. Instr. Meth. A 483(2002)94. [7] S. Biedron et al., Phys. Rev. ST 5(2002)030701. [8] Z. Huang and K. Kim, Phys. Rev. E, 62(2000)7295. [9] Z. Huang and K. Kim, Nucl. Instr. Meth. A 475(2001)112. [10] A. Tremaine et al., Phy. Rev. Lett. 88, 204801 (2002) [11] W. Brefeld et al., Nucl. Instr. Meth. A 507(2003)431.

[12] E.L. Saldin, E.A. Schneidmiller, and M.V. Yurkov, Nucl. Instr. Meth. A 429(1999)233.

[13] R. Bonifacio, C. Pellegrini and L.M. Narducci, Opt. Commun. 50(1984)373. [14] E.L. Saldin, E.A. Schneidmiller, and M.V. Yurkov, The Physics of Free Electron Lasers, Springer-Verlag, Berlin, 1999.

[15] W.M. Fawley, Phys. Rev. STAB, 5(2002)070701.

[16] E.L. Saldin, E.A. Schneidmiller, and M.V. Yurkov, Opt. Commun.

148(1998)383.

[17] E.L. Saldin, E.A. Schneidmiller, and M.V. Yurkov, Opt. Commun.

212(2002)377.

[18] J. Goodman, Statistical Optics, Willey, New York, 1985. [19] H. Wiedemann, Synchrotron Radiation, Springer-Verlag, Berlin, 2003.